ტექნიკური დავალების ფორმა

დანართი #1

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **#** | **Ref.** | **Article** | **Description** | **Datasheet** | **Image** | **Dimensions** | **DIM Type** | **Manufacturer** | **Q-ty** | **Price USD,**  **VAT incl.** | **Total, USD,**  **VAT incl.** |
| 1 | **LS01** | BH11-11W9F2OS14 | Downlight Nit Round Fix ø105 13.4W LED warm- white 3000K CRI 92 56.5º ON-OFF White IN IP20 / OUT IP54 1509lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/BH11-11W9F2OS14.html) [c4.com/ft2/en/BH11-](https://files.leds-c4.com/ft2/en/BH11-11W9F2OS14.html) [11W9F2OS14.html](https://files.leds-c4.com/ft2/en/BH11-11W9F2OS14.html) | https://files.leds-c4.com/main-photo/BH11-11W9F2OS14 |  | ON/OFF | LedsC4 | 296.00 |  |  |
| 2 | **LS02** | BH12-27W9F2OS14 | Downlight Nit Round Fix ø150 30.9W LED warm- white 3000K CRI 92 63.7º ON-OFF White IN IP20 / OUT IP54 3457lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/BH12-27W9F2OS14.html) [c4.com/ft2/en/BH12-](https://files.leds-c4.com/ft2/en/BH12-27W9F2OS14.html) [27W9F2OS14.html](https://files.leds-c4.com/ft2/en/BH12-27W9F2OS14.html) | https://files.leds-c4.com/main-photo/BH12-27W9F2OS14 |  | ON/OFF | LedsC4 | 144.00 |  |  |
| 3 | **LS03** | 15-7192-14-MS | Ceiling fixture Bento Surface 6 LEDS 14.7W LED warm-white 3000K CRI 92 Phase cut (trailing edge) White IP23 1326lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/15-7192-14-MS.html) [c4.com/ft2/en/15-7192-14-](https://files.leds-c4.com/ft2/en/15-7192-14-MS.html) [MS.html](https://files.leds-c4.com/ft2/en/15-7192-14-MS.html) | https://files.leds-c4.com/main-photo/15-7192-14-MS |  | ON/OFF | LedsC4 | 79.00 |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 4 | **LS04** | 15-7169-14-60 | Ceiling fixture Bento Surface 3 LEDS 6.1W LED warm-white 3000K CRI 92 White Black IP23 663lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/15-7169-14-60.html) [c4.com/ft2/en/15-7169-14-](https://files.leds-c4.com/ft2/en/15-7169-14-60.html) [60.html](https://files.leds-c4.com/ft2/en/15-7169-14-60.html) | https://files.leds-c4.com/main-photo/15-7169-14-60 |  | ON/OFF | LedsC4 | 43.00 |  |  |
| 5 | **LS04** | 71-B232-00-00 | Driver Driver On-Off 9W 700mA | [https://files.leds-](https://files.leds-c4.com/ft2/en/71-B232-00-00.html)  [c4.com/ft2/en/71-B232-00-](https://files.leds-c4.com/ft2/en/71-B232-00-00.html) [00.html](https://files.leds-c4.com/ft2/en/71-B232-00-00.html) | https://files.leds-c4.com/main-photo/71-B232-00-00 |  | ON/OFF | LedsC4 | 43.00 |  |  |
| 6 | **LS07** | DE-0131-BLA | Downlight FAB GU10 8W White | [https://files.leds-](https://files.leds-c4.com/ft2/en/DE-0131-BLA.html) [c4.com/ft2/en/DE-0131-](https://files.leds-c4.com/ft2/en/DE-0131-BLA.html) [BLA.html](https://files.leds-c4.com/ft2/en/DE-0131-BLA.html) | https://files.leds-c4.com/main-photo/DE-0131-BLA |  | ON/OFF | LedsC4 | 30.00 |  |  |
| 7 | **LS07** |  | Bulb  1xGU10x8W |  |  |  |  |  | 30.00 |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | **LS08** | 15-A070-14-TS | Spotlight Atom Surface ø52 14.3W LED warm- white 3000K CRI 92 42.7º PHASE CUT White 1316lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/15-A070-14-TS.html) [c4.com/ft2/en/15-A070-14-](https://files.leds-c4.com/ft2/en/15-A070-14-TS.html) [TS.html](https://files.leds-c4.com/ft2/en/15-A070-14-TS.html) |  |  | ON/OFF | LedsC4 | 4.00 |  |  |
| 9 | **LS09** |  | Bulb  1xE27x70W |  |  |  | ON/OFF | LedsC4 | 10.00 |  |  |
| 10 | **LS10** | 90-A027-14-00 | Downlight Lite Deep Fix ø70mm 8.5W LED warm- white 3000K CRI 92 34º ON-OFF White IP54 667lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/90-A027-14-00.html) [c4.com/ft2/en/90-A027-14-](https://files.leds-c4.com/ft2/en/90-A027-14-00.html) [00.html](https://files.leds-c4.com/ft2/en/90-A027-14-00.html) |  |  | ON/OFF | LedsC4 | 132.00 |  |  |
| 11 | **LS11** | 19.4073.2241.34 | AGAT CLEAN LED CRI95 3600 PLX E IP65 940 / 600X300 | https://luxiona.pl/en/offer/cle an-luminaires-cri95/agat-clean- led-cri95/19.4073.2141.34/ |  |  | ON/OFF | LUXIONA | 23.00 |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 12 | **LS12** | TC-0083-BLA | Downlight Element Ø145mm LED 11.5W SW 3000-  4000-6000K ON-OFF White IN IP20 / OUT IP54  1890 | [https://files.leds-](https://files.leds-c4.com/ft2/en/TC-0083-BLA.html) [c4.com/ft2/en/TC-0083-](https://files.leds-c4.com/ft2/en/TC-0083-BLA.html) [BLA.html](https://files.leds-c4.com/ft2/en/TC-0083-BLA.html) |  |  | ON/OFF | LedsC4 | 17.00 |  |  |
| 13 | **LS13** | 91-7909-00-00 | LED strip On Basic 4,8 8mm 24W LED warm-white 3000K CRI 80 IP20 2524lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/91-7909-00-00.html) [c4.com/ft2/en/91-7909-00-](https://files.leds-c4.com/ft2/en/91-7909-00-00.html) [00.html](https://files.leds-c4.com/ft2/en/91-7909-00-00.html) |  |  | ON/OFF | LedsC4 | 79.00 |  |  |
| 14 | **LS13** | 71-8130-54-M3 | Lineal lighting system Lineal Anodised aluminium IP20 | [https://files.leds-](https://files.leds-c4.com/ft2/en/71-8130-54-M3.html) [c4.com/ft2/en/71-8130-54-](https://files.leds-c4.com/ft2/en/71-8130-54-M3.html) [M3.html](https://files.leds-c4.com/ft2/en/71-8130-54-M3.html) |  |  | ON/OFF | LedsC4 | 197.00 |  |  |
| 15 | **LS13** | 71-B642-00-00 | Power source Power Supply On-Off 24V 150W ON- OFF | [https://files.leds-](https://files.leds-c4.com/ft2/en/71-B642-00-00.html) [c4.com/ft2/en/71-B642-00-](https://files.leds-c4.com/ft2/en/71-B642-00-00.html)  [00.html](https://files.leds-c4.com/ft2/en/71-B642-00-00.html) |  |  | ON/OFF | LedsC4 | 63.00 |  |  |
| 16 | **LS14** | 91-7917-00-00 | LED strip On Basic 9,6 8mm 48W LED warm-white 3000K CRI 80 IP20 5113lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/91-7917-00-00.html) [c4.com/ft2/en/91-7917-00-](https://files.leds-c4.com/ft2/en/91-7917-00-00.html) [00.html](https://files.leds-c4.com/ft2/en/91-7917-00-00.html) |  |  | ON/OFF | LedsC4 | 2.00 |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 17 | **LS14** | 71-8130-54-M3 | Lineal lighting system Lineal Anodised aluminium IP20 | [https://files.leds-](https://files.leds-c4.com/ft2/en/71-8130-54-M3.html) [c4.com/ft2/en/71-8130-54-](https://files.leds-c4.com/ft2/en/71-8130-54-M3.html) [M3.html](https://files.leds-c4.com/ft2/en/71-8130-54-M3.html) |  |  | ON/OFF | LedsC4 | 4.00 |  |  |
| 18 | **LS14** | 71-B642-00-00 | Power source Power Supply On-Off 24V 150W ON- OFF | [https://files.leds-](https://files.leds-c4.com/ft2/en/71-B642-00-00.html)  [c4.com/ft2/en/71-B642-00-](https://files.leds-c4.com/ft2/en/71-B642-00-00.html) [00.html](https://files.leds-c4.com/ft2/en/71-B642-00-00.html) |  |  | ON/OFF | LedsC4 | 1.00 |  |  |
| 19 | **LS15** | BH11-11X9F2OS14 | Downlight Nit Round Fix ø105 13.4W LED neutral- white 4000K CRI 92 56.5º ON-OFF White IN IP20 / OUT IP54 1533lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/BH11-11X9F2OS14.html) [c4.com/ft2/en/BH11-](https://files.leds-c4.com/ft2/en/BH11-11X9F2OS14.html) [11X9F2OS14.html](https://files.leds-c4.com/ft2/en/BH11-11X9F2OS14.html) |  |  | ON/OFF | LedsC4 | 27.00 |  |  |
| 20 | **LS16** | 19.4073.2141.34 | AGAT CLEAN LED CRI95 3600 PLX E IP65 940 / 600X300 | https://luxiona.pl/en/offer/cle an-luminaires-cri95/agat-clean- led-cri95/19.4073.2141.34/ |  |  | ON/OFF | LedsC4 | 15.00 |  |  |
| 21 | **LS17** | AK11-15W8PMDS14 | Lineal lighting system Infinite Pro 854mm Surface Opal 13.8W LED warm-white 3000K CRI 80 DALI- 2/PUSH White IP40 2131lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/AK11-15W8PMDS14.html) [c4.com/ft2/en/AK11-](https://files.leds-c4.com/ft2/en/AK11-15W8PMDS14.html) [15W8PMDS14.html](https://files.leds-c4.com/ft2/en/AK11-15W8PMDS14.html) |  |  | ON/OFF | LedsC4 | 36.00 |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 22 | **LS18** | TC-0472-BLA | Downlight Bala Ø82mm LED 8.9W LED warm-  white 3000K PHASE CUT White IP65 850.00 | [https://files.leds-](https://files.leds-c4.com/ft2/en/TC-0472-BLA.html) [c4.com/ft2/en/TC-0472-](https://files.leds-c4.com/ft2/en/TC-0472-BLA.html) [BLA.html](https://files.leds-c4.com/ft2/en/TC-0472-BLA.html) |  |  | ON/OFF | LedsC4 | 8.00 |  |  |
| 23 | **LS19** | 05-9911-Z5-CM | Wall fixture IP65 Afrodita LED 220mm Double Emission LED 17.9W LED neutral-white 4000K ON- OFF Urban grey 1644lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/05-9911-Z5-CM.html) [c4.com/ft2/en/05-9911-Z5-](https://files.leds-c4.com/ft2/en/05-9911-Z5-CM.html) [CM.html](https://files.leds-c4.com/ft2/en/05-9911-Z5-CM.html) |  |  | ON/OFF | LedsC4 | 45.00 |  |  |
| 24 | **LS20** | 90-6369-14-60 | Downlight Bento Standard 3 LEDS Trim 6.1W LED warm-white 3000K CRI 92 47.7º White Black IP23 663lm | [https://files.leds-](https://files.leds-c4.com/ft2/en/90-6369-14-60.html) [c4.com/ft2/en/90-6369-14-](https://files.leds-c4.com/ft2/en/90-6369-14-60.html) [60.html](https://files.leds-c4.com/ft2/en/90-6369-14-60.html) |  |  | ON/OFF | LedsC4 | 8.00 |  |  |
| 25 | **LS20** | 71-B232-00-00 | Driver Driver On-Off 9W 700mA | [https://files.leds-](https://files.leds-c4.com/ft2/en/71-B232-00-00.html) [c4.com/ft2/en/71-B232-00-](https://files.leds-c4.com/ft2/en/71-B232-00-00.html)  [00.html](https://files.leds-c4.com/ft2/en/71-B232-00-00.html) |  |  | ON/OFF | LedsC4 | 8.00 |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 26 | **LS23** |  | Bulb 1xE27x70W | #N/A |  |  | ON/OFF | LedsC4 | 4.00 |  |  |
|  | | | | | | | | | Grand Total, USD, VAT incl. | |  |